Classical CAN Devices:
         CAN-PCIe/402, CAN-PCI/402, PMC-CAN/402, XMC-CAN/402,
         CPCIserial-CAN/402-4, CPCI-CAN/402-4, CAN-PCIeMini/402

CAN FD Devices:
         CAN-PCIe/402-FD, CAN-PCI/402-FD, PMC-CAN/402-FD, XMC-CAN/402-FD,
         CPCIserial-CAN/402-4-FD, CPCI-CAN/402-4-FD, CAN-PCIeMini/402-FD
         CAN-M.2/402, CAN-PCIeMiniHS/402, PMC-CAN/402-FD-LIN-DIO,
         XMC-CAN/402-FD-LIN-DIO

This folder contains the following additional tools for these CAN interfaces
All tools are 32-bit binaries which also work without any restrictions on
64-bit versions of Windows.

Firmware Update:

updc402fd.exe  - Firmware update tool for the CAN C402 FD Hardware Family to
                  (FW 00.77 (dec) / 00.4D (hex))

updc402.exe    - Firmware update tool for the Classical CAN C402 Hardware
                 Family to (FW 00.77 (dec) / 00.4D (hex))

               Please refer to chapter 5 of the "NTCAN Installation Manual"
               for a description of the FW update process.
               NOTE: A cross-update to turn a Classical CAN interface into
                     a CAN FD device and vice versa is not possible.
                
_____________________________________________________________________
© esd electronic system design gmbh 2000-2025

          esd electronics gmbh
       Vahrenwalder Str. 207

     30165 Hannover, Germany
    Phone: +49-511-372 98-0
   Fax: +49-511-372 98-68
  E-mail: info@esd.eu
 Internet: www.esd.eu
_____________________________________________________________________

Document Number: SD31200