Update process of the CAN-PN/2 | CAN-PN/2-FD | CANopen-PN/2

1. Connect the gateway via Mini-USB with a PC.
2. Open the 'Device Manager' and check if a new serial device have been detected.
3. Install the RNDIS driver for the device
4. Check if a new 'Network adapter' called 'RNDIS based ESD Device' is detected.
5. Execute the 'update.bat' and press 1 and enter for update.
6. The LED 'R' of the gateway device starts blinking.
7. The update process can take several minutes. The device will restart automatically when the update is finished. 
	DO NOT power down the device during the process even if the Windows 'CMD'-Window is finished.

